1. Create new project -> create new block design

2. add these blocks:

a. zynq7 processing system

i. run block automation and do the DDR and FIXED\_IO connections

ii. double click PS -- PS-PL configuration -> GP Master AXI Interface -> M AXI GP0 Interface and make sure its checked

b. reset for ps


c. axi interconnect

d. axi bram ctrl

i. double click it and changed number of BRAM interfaces to 1 and change to AXI4LITE

3. After all this is added, run connection automation, press regenerate layout to reorder components (\*makes it look neater), press validate design and make sure no errors.

4. You should have this after doing everything above, if not, connect all the wires manually and validate design:



5. Tools -> create and package new IP -> new AXI peripheral -> create a name you will remember -> edit IP on the last step and press finish

6. in the package IP vivado -> add all the design sources

7. add this in, the \_v1\_0.v file, if you are unsure about this step, refer to the github where its uploaded:

a. At line 7:

parameter WIDTH=32, SIZE=512, //WIDTH is bits per word(shouldn't be changed), SIZE is # of WORDS

parameter NUM\_COL = 4,

parameter COL\_WIDTH = 8,

localparam integer LOGSIZE=$clog2(SIZE),

b. at line 49 add: wire ps\_reset;

c. add this inside the instantiation .ps\_reset(ps\_reset)

d. output ps\_reset, -> add at line 18

assign ps\_reset = slv\_reg0; -> add this to line 117

